<xml version="0.99" board="Arduino Uno"><block type="controls_if" id=")p0RrjE=#cO+lGc#[uDS" x="-1053" y="5"><value name="IF0"><block type="logic_negate" id="G4#9Mc^=@J7RLhONQESP"><value name="BOOL"><block type="inout_digital_read2" id=";![8TkV8KBbfZPO22Qsx"><value name="PIN"><shadow type="pins_digital" id="#GPeM{zXU2w;mk@~2?Y_"><field name="PIN">2</field></shadow></value></block></value></block></value><statement name="DO0"><block type="base_delay" id="1Kmt:*6@x(^?uK%LaO{x"><field name="UNIT">delay</field><value name="DELAY_TIME"><shadow type="math_number" id="FuqpQyAIHe5S~HY-^u(D"><field name="NUM">10</field></shadow></value><next><block type="controls_if" id="vnG4#}U]kOrZq`_{eZ/l"><value name="IF0"><block type="logic_negate" id="8/]`+Ah1-d,?`0bPTBH%"><value name="BOOL"><block type="inout_digital_read2" id="z8bo:(wqaI,peOO6]R1h"><value name="PIN"><shadow type="pins_digital" id="^U%p=r[xNaS^bJw?6*wP"><field name="PIN">2</field></shadow></value></block></value></block></value><statement name="DO0"><block type="serial_write" id="9z))Bt}.C[wEmJZ!`;N0"><field name="serial_select">Serial</field><value name="CONTENT"><block type="math_number" id="F@@qYo4=z0X7A*6)Q1%T"><field name="NUM">0x83</field></block></value><next><block type="serial_write" id="=NYPLbq2XUGj@M?ljlT{"><field name="serial_select">Serial</field><value name="CONTENT"><block type="math_number" id="{K#6`L)N)?hVwdW=aM?D"><field name="NUM">0x1b</field></block></value></block></next></block></statement><next><block type="controls_whileUntil" id="i%l|U1`PxQg5l@D~Sh7="><field name="MODE">WHILE</field><value name="BOOL"><block type="logic_negate" id="Be0qQLYyLF4nzq1~o.TT"><value name="BOOL"><block type="inout_digital_read2" id=")pJi*[aHJSdYvzQ=Bh3{"><value name="PIN"><shadow type="pins_digital" id="@p8Sj-B(k[0c:,bR-tcA"><field name="PIN">2</field></shadow></value></block></value></block></value></block></next></block></next></block></statement></block></xml>